===================================================================
Avaya Inc                                                  May 2002
NDIS 4 Miniport Driver for MS-Windows NT4   Variant 1 Version: 7.62
===================================================================

This README.TXT covers information that was not yet known or
available when the user documentation shipped with this product
was written. It includes update information, additional
installation instructions, limitations to the current version of
the product, and suggestions to solve known issues or problems.

TABLE OF CONTENTS.

1.  SOFTWARE DESCRIPTION
2.  SYSTEM REQUIREMENTS
3.  NEW IN THIS RELEASE
4.  INSTALLATION NOTES
5.  TECHNICAL CONSTRAINTS
6.  KNOWN ISSUES
7.  TECHNICAL SUPPORT

-------------------------------------------------------------------

1.  SOFTWARE DESCRIPTION

1.1 About this software
    This Driver supports the following network interface cards:
     * "Wireless PC Card Model 0104"
     * "Wireless PC Card Model 0106"
     * "Wireless Integrated Card Model 0202"
     * "Wireless Embedded Card Model 0504"
     * "Wireless PCI Adapter Model 0901"
     * "Avaya Wireless PC Card"
     * "NCR WaveLAN/IEEE PC Card"
     * "ELSA AirLancer MC-11"
     * "ELSA Vianect WLAN MC-11"
     * "IBM High Rate Wireless LAN PC Card"
     * "IBM High Rate Wireless LAN Mini PCI Card"
     * "IBM Internal High Rate Wireless LAN PC Card"
     * "ORiNOCO PC Card (5 volt)"
     * "ORiNOCO Mini PCI Card"
     * "ORiNOCO Integrated Card"
     * "ORiNOCO PCI Card"
     * "Toshiba Wireless LAN Card"
     * "Toshiba Wireless LAN Mini PCI Card"
     * "Samsung SEW-2001p Card"
     * "Samsung SEW-2001m Card"
     * "I-GATE 11M PC Card"
     * "connect2AIR WLAN E-1100 PC-Card"
     * "Tyco Electronics 802.11b Card"
     * "2Wire Wireless PC Card"
     * "WLAN PC Card"
     * "WLAN Integrated Card"
     * "WLAN Embedded Card"

1.2 Files Installed
    The following files will be installed in the Windows designated
    directory:

    NDIS 4 Miniport driver for Windows NT4            version 7.62
        WLAGS52.SYS
        OEMSETUP.INF
        WCAGS52.EXE
        WNAGS52.CPL
        WAAGS52.DLL
        WNAGS.HLP
        WNAGS.CNT

-------------------------------------------------------------------

2.  SYSTEM REQUIREMENTS

2.1 Operating System
    This Driver is for the Microsoft Windows NT4 Operating System.

-------------------------------------------------------------------

3.  NEW IN THIS RELEASE

3.1 Version 7.62                                           May 2002
      * For each OS a multi-brand INF file is generated.
        As the name suggests, a multi-brand INF file contains
        the card characteristics of various brands.
        Multi-brand must not be confused with Combined, the latter
        representing the card characteristics on various OS’es 
        for one brand.
      * Various inconveniences w.r.t. Japanese help files
        and screen texts have been resolved
      * Stability issues have been resolved for
        the Control Panel Applet
      * Firmware 8.42 is used in the driver.
        - Initial value for CurrentTXRate is 11 Mbps i.s.o. 2 Mbps.
        - Led behaviour has been modified:
          Power led off:                      radio disabled
          Power led continuously on:          radio enabled
          Power led flickers every 100 ms:    radio enabled and
                                              power management ON
          Activity led off                    radio disabled
          Activity led flickers once per 10s: radio enabled
                                              but no network found
          Activity led flickers every 100 ms: radio enabled and
                                              Rx/Tx activity

3.2 Version 7.42                                        Winter 2002
      * Added support for
        - 802.1x authentication
        - Ultra high density
        - Promiscuous mode
        - PCI Adapter Card

      * Extended functionality of Control Panel Applet
        The Control Panel Applet has been extended such that it 
        supports multiple cards to be configured in a single 
        system.

      * Agere-ization has been performed, involving
        replacement of Lucent-related texts to Agere equivalent.

3.3 Version 7.08                                          Fall 2001
      * Correct problem: Control Panel Applet does not accept
        hexadecimal coded encryption keys.

3.4 Version 7.06                                        Summer 2001
      * Added Firmware as part of the driver.
      * Changed ControlPanel to Wizard style
      * Added Enhanged PowerManagement

3.5 Version 6.28                                        Winter 2001
      * Added functionality for enabling/disabling radio from the
        Client Manager 
      * Putting 'ANY' in a peer-to-peer profile gives a apropriate 
        warning.
      * Profiles can now be selected trough the keyboard.

-------------------------------------------------------------------

4.  INSTALLATION NOTES

4.1 Standard Installation
    Please refer to the 'Getting Started Guide' or 'User's
    Guide' that came with your product.

    During installation, after giving driver path and NT files
    path, the network installation will ask the user to reboot
    the system. This only appears to be a problem when a clean
    install of the OS is done and network components are
    installed for the first time.

    You can resolve this error by answering NO
    to the first question to reboot the system after installing
    the driver files. Only reboot the system after the Network
    Install Wizard has Finished. 

-------------------------------------------------------------------

5.  TECHNICAL CONSTRAINTS

5.1 Compatibility with Station Functions Firmware on the Card.
    This version of the driver requires the Station Functions
    firmware on the Card to be version 6.04 or higher.

-------------------------------------------------------------------

6.  KNOWN ISSUES

6.1 "Wireless" Add/Edit profile does not appear upon installation

    The "Wireless" driver requires Windows NT Service Pack 4 or
    higher.

    In case you are running SP3 or lower, your Windows NT system
    does not provide the Windows system DLLs required to make the
    Add/Edit profile window work.

    You can resolve this error by either:
    * Installing Microsoft Windows NT Service Pack 4 or higher
      (SP 6 is recommended), 
    * (Re-)installing the latest Client Manager.

6.2 I/O Port conflicts under MS-Windows NT4.

    When your "Wireless" Card's installation completed successfully,
    but it does not become operational, you are advised to try a
    different I/O Port value.

6.3 IRQ conflicts under MS-Windows NT4.

    When your "Wireless" Card's installation completed successfully,
    but it does not become operational, you are advised to try a
    different IRQ value.

-------------------------------------------------------------------

7.  TECHNICAL SUPPORT


7.1 Finding Information
    Consult your authorized reseller or manufacturer for more
    information. Alternately consult our the Avaya Wireless Support
    Web Site for the most recent device drivers and software updates 
    and user documentation.

    World Wide Web:    HTTP://SUPPORT.AVAYA.COM

7.2 Contact Technical Support
    If you encounter problems when installing or using this
    product, or would like information about our other
    Wireless products, please contact your local Authorized
    Wireless Reseller or Avaya Sales office.
   
    Addresses and telephone numbers of the Avaya Systems
    Sales offices are listed on WWW.AVAYA.COM.
===================================================================
                          END OF FILE
