===========================================================
Avaya Wireless                                 Spring  2001
Windows CE Software for Avaya Wireless PC Cards
===========================================================

This README.TXT covers information that was not yet known 
or available when the user documentation for this product
was written. This text file includes update information, 
additional installation instructions, limitations to the 
current version of the product, and suggestions to solve
known issues or problems.


TABLE OF CONTENTS.

1.  SOFTWARE DESCRIPTION
2.  SYSTEM REQUIREMENTS
3.  NEW IN THIS RELEASE
4.  INSTALLATION NOTES
5.  TECHNICAL CONSTRAINTS
6.  KNOWN ISSUES
7.  TECHNICAL SUPPORT
        
-----------------------------------------------------------
1.  SOFTWARE DESCRIPTION

1.1 Description 

    This software is officially released and supported 
    software of Avaya Communication Inc. 

1.2 Software Components
    This software for Avaya Wireless PC Cards comprises the
    following components:

    Windows CE Driver v 6.28 and Client Manager v 1.02
        Handheld PC 2000 and Pocket PC (WinCE 3.0).
        WinCE 2.12 
        Handheld PC Pro (WinCE 2.11)
    Windows CE Driver v 4.06
        Handheld PC (WinCE 2.10).
        WinCE 2.00 

    These components can be installed by running the following 
    setup programs from CD:\Drivers\Win_CE\ or the drive that 
    you specify during the extraction of the downloaded file.

    Pocket PC -          \PocketPC\Setup.exe
    Handheld PC 2000 -   \HPC2000\Setup.exe
    WinCE 2.12 -         \WinCE212\Setup.exe
    Handheld PC Pro -    \Win_CE\HPCPro\Setup.exe
    Handheld PC -        \HPC\Setup210.exe
    WinCE 2.00 -         \WinCE200\Setup200.exe


1.3 Software Versions
    The following software will be installed on the Windows CE 
    device during setup:
   
    Windows CE Driver v 6.28 and Client Manager v 1.02
	Name: WLLUC46.DLL
	Name: WRLUC46.DLL
	Name: WCLUC46.CPL
	Name: WCLUC46.EXE
	Name: WMLUC46.EXE
	Name: WNCON46.HTM
	Name: WNEDT46.HTM
	Name: WNIDX46.HTM

    Windows CE Driver v 4.06
	Name: wvlan46.dll
	Name: wvlan.cpl
	Name: w4600000.htp ... w46000047.htp 
	Name: wavelan.htc

1.4 Other Files included 
    Readme file (this file):     README.TXT  (Plain text format)
    End-User License Agreement:  LICENSE.TXT (Plain text format)
    Problem Report Form:         REPORT.TXT  (Plain text format)

-----------------------------------------------------------
2.  SYSTEM REQUIREMENTS

2.1 Operating System
    The software and/or drivers provided on this diskette
    can be installed on the operating systems 
    * Windows CE 2.0, 2.11 and 2.12.
    * Windows CE 3.0

2.2 Free Disk Space
    To install and run the software you will need 280KB
    of free disk space on your Windows CE Device.

2.3 RAM 

2.4 Certified Notebooks

    Windows CE 3.0 
    * Compaq iPAQ 

    Windows CE 2.11
    * Sharp Tripad 
    * NEC Mobilon PRO 770 
    * HP Jornada 820 

    Windows CE v2.0 (HPC) systems 
    * Compaq 2010 
    * HP 620 
    * HP 660 
    * NEC Mobilon PRO 750 

-----------------------------------------------------------
3.  NEW IN THIS RELEASE

3.1 Version 6.28

    * Initial Avaya Wireless Release.

-----------------------------------------------------------
4.  INSTALLATION NOTES

4.1 Before you start

    The MS-Windows CE operating system exists in various 
    versions, and runs on different processor types. 
    Prior to installation check which version of 
    Microsoft Windows CE and processor are used by your
    device:

    1.  Power up your device.
    2.  Click the Start button on the Windows Taskbar.
    3.  Point to Settings, and select "Control Panel".
    4.  On the control Panel:
        a)  Check if the panel includes the icon "Wireless Network"
            (if it does not appear, consult section 5.1 of
            this readme.txt file).
        b)  Double-click the icon "System" to display the
            System properties.

            To be able to use the Avaya Wireless PC Card with your
            device using the current driver, your handheld
            device must match the following requirements:

            *   Microsoft Windows CE v2.00, v2.11, v2.12 or v3.00
            *   Processor Type: 
            - MIPS, SH3 and X86 for WinCE 2.00
            - SH4, ARM and X86 for WinCE 2.11 and 2.12
		- SH3, SH4, MIPS, ARM and x86 for Handheld PC 2000
            - SH3, MIPS, ARM for PocketPC

4.2 Install the software

    Handheld PC (HPC) devices running Windows CE are typically 
    used in combination with another computer running 
    "Windows CE Services" to transfer data between this computer
    and your handheld device.

    To install the Avaya Wireless software on your handheld device you 
    will need to:

    1.   Run the setup file on the computer that has the 
         "Windows CE Services" installed.

    2.  Next use the serial cable or docking station of your 
        handheld device, to connect your device to the computer
        that you used to install the software. 

    3.  Once connected, the "Windows CE Services" should 
        automatically transfer the files from the computer to 
        your handheld device.

    4.  Insert the Avaya Wireless PC Card or, if already inserted, 
        eject and reinsert it.

    5.  After first time installation use the Control Panel 
        Applet to configure your wireless profiles.


4.3 Configuration of the Avaya Wireless Driver

    When you insert your Avaya Wireless PC Card the Avaya Wireless
    Client should startup automatically. The icon of the Avaya 
    Wireless Client can be seen on the task bar, click this icon 
    to show the Client. From the Client you can start the 
    configuration program of the Avaya Wireless driver.

    Alternatively, you can configure the Avaya Wireless Driver by
    clicking the Wireless Network icon in the Control Panel.
    Consult the documentation you received with your Windows 
    CE Device if you don not know how to open the Control Panel.

    Detailed Installation and configuration procedures are 
    described in the online copy of the 'PC Card User's Guide' 
    that came with your Avaya Wireless product. 

    Avaya Wireless User documentation is also available in 
    electronic format on the Avaya Wireless Web Site.
    (http://www.avaya.com/).
    You can download the documentation in Adobe's Acrobat
    Portable Document Format (PDF). To view or print PDF
    files you will need the freeware Acrobat Reader that 
    can be downloaded from the Adobe Web Site 
    (http://www.adobe.com/acrobat).

4.4 Windows CE Services

    For more information about Windows CE Services, please 
    consult the Microsoft Handheld PC Companion booklet 
    and/or the user documentation of your handheld device.

-----------------------------------------------------------
5.  TECHNICAL CONSTRAINTS

5.1 Unable to use internet explorer.

    Description: When trying to brows the internet with internet
                 explorer you get the error message "The page 
                 you are looking for cannot be found".

    Impact:      After installing the software on the device
                 you are unable to brows the internet with
                 internet explorer on your Windows CE device. 

    Action:      * Make sure your Network are configured correctly.
                   You can do this by clicking the "Network" icon in
                   the control panel.
                 * Make sure your proxy server is configured correctly.
                   Do this by clicking Tools/Options/Connections" in
                   internet explorer.
                 * Make sure you have entered your password correctly
                   in the "Wireless Network" configuration. If the 
                   password is spelled incorrectly the Avaya Wireless 
                   Client will show a good connection but no communication
                   will be possible.
                 * Disconnect your Windows CE device from your PC and
                   try again.

5.2 Device does not show the "Wireless Network" Icon
    in the control panel.

    Description: After installing the software on the device
                 the "Wireless Ntwork" icon is not displayed 
                 in the Control Panel.

    Impact:      You will not be able to configure the card 
                 from the control panel. 

    Action:      Some devices might require a reset after 
                 installation before the "Wireless Network" 
                 icon becomes visible in the Control Panel.

5.3 Device does not show the Network Icon

    Description: On some Handheld PC devices running the
                 MS-Windows CE v2.00 operating system
                 the files required to support network 
                 connectivity have not been pre-installed.
		     
                 To determine if network connectivity have 
                 not pre-installed open the "Control Panel" 
                 of your handheld device and look for the 
                 "Network" icon. If this icon is missing 
                 you will need to run the additional 
                 installation file called "netsetup.exe" 
                 prior to installing the WaveLAN driver 
                 software.

    Impact:      If these networking files are missing, you
                 will not be able to establish a network
                 connection using a network adapter card 
                 like the Avaya Wireless PC Card.

    Action:      The installation file "netsetup.exe"
                 will add the 'WinCE 2.0 Additional Network 
                 Components' if they were not pre-installed
                 on your handheld device by the hardware 
                 manufacturer.

                 Optionally, you may check the CD-ROM or disk
                 that came with your device for the same file.
                 
                 On some devices you may need to "RESET" the 
                 device using the special reset button of the 
                 bottom of the device before the Network icon 
                 will display correctly.

                 Consult the documentation of your handheld 
                 device to locate the reset button.

5.4  HPC device does not show the "Wireless Settings" Icon

    Description: On some Handheld PC devices running the
                 MS-Windows CE v2.00 operating system
                 the WaveLAN icon does not show up after
                 installing the Avaya Wireless driver.

    Impact:      This is caused by the fact that the device
                 does not have the file "MFCCE20.DLL" 
                 pre-installed, which is required to display
                 and run the WaveLAN driver configuration 
                 panel.

    Action:      Use the Windows CE Services to copy the
                 "MFCCE20.DLL" from the Avaya Wireless CD-ROM
                 to the system folder of your handheld device.

                 Remove and re-insert the Avaya Wireless PC
                 Card to verify if the "Wireless Settings" icon 
                 displays correctly.

                 You may need to restart the device to 
                 allow the MS-Windows CE system to load the
                 file correctly.

5.5 WaveLAN PC Card Hardware Compatibility

    Description: All Avaya Wireless PC Cards are backwards compatible
                 with previously marketed WaveLAN PC Cards.
                 You can use all Avaya Wireless PC Cards inside a
                 handheld device running Windows CE.
                 
                 WaveLAN PC Cards manufactured between 
                 June and September 1998 have a hardware
                 design that is not compatible with the
                 Windows CE driver.

    Impact:      WaveLAN PC Cards with a Serial Number 
                 lower than 98UT08333219 can not be used
                 in devices running Windows CE.

                 The Serial Number of the card is printed 
                 on a label on the back-side of the WaveLAN
                 PC Card.
                 
                 This type of cards can however be used
                 without problems in any other supported
                 operating system (Windows 95/98/NT and/or
                 MS-DOS, Apple & Linux).

    Action:      You are advised to:
                 * Only use cards with Serial Number 
                   98UT08333219 or higher in handheld 
                   devices running Windows CE.
                 * Use cards with Serial Number 98UT08333218
                   or lower only in computers that run the
                   Windows 95/98/NT/2000, MS-DOS, Apple or
                   Linux operating system.

                   In this type of operating systems the 
                   cards will run without any difficulty.

-----------------------------------------------------------
6.  KNOWN ISSUES
    At the time of release of this software, the following 
    problems remain to be solved:


6.1 No known issues

-----------------------------------------------------------
7.  TECHNICAL SUPPORT

7.1 Finding Information
    On the Avaya Wireless  Web Site you can find the most
    recent device drivers, bridge firmware, software updates and 
    user documentation. 

    World Wide Web:    HTTP://WWW.AVAYA.COM

7.2 Contact Technical Support
    If you encounter problems when installing or using this
    product, or would like information about our other 
    Avaya Wireless products, please contact your local Authorized
    Avaya Wireless Reseller or Sales office.
   
    Addresses and telephone numbers of the Sales offices 
    are listed on our Web Site.

    When contacting Technical Support, please use 
    the Problem Report Form and send it to us by Fax or 
    E-Mail. The Problem Report Form 'REPORT.TXT'
    (Plain text format) is included with the software diskette, or 
    downloaded set of files.
    Alternatively, you can download the Problem Report Form
    from our Web Site.

    Include Product Name, Serial Number and software 
    version number with each request to help the Technical
    Support Group helping you.

===========================================================
                          END OF FILE


